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	TOOLS
	
	TOOL CLEANING
	

	
	Plastic or metal spatula.

	
	Clean all tools immediately after use with warm water and soap. Do not dispose of washing waste water into the aquifer.
	

	
	PACKAGING
	
	STORAGE
	

	
	Available in 1lt plastic containers.
	
	Store original, sealed containers in dry place at temperatures between +5°C and +35°C for a long period of time.
	

	
	TEMPERATURE
	
	
	

	
	Do not apply when temperatures are below 5ºC. Adverse conditions during or shortly after application may affect the
	
	final properties of the product.
	

	
	PRECAUTIONS
	
	
	

	
	For information on the safe use, storage and disposal of the product read the information on the label and in the most recent Product Safety Data Sheet. The Product Safety Data Sheet is available at the professionals’ request. Remaining 

	
	paint should not be disposed of with household waste. You should seek advice from local authorities regarding the disposal and collection of waste.
Poisons Information Call Center 210 77.93.777

	

	
	

	
	TECHICAL SPECIFICATIONS
	UNITS
	STANDARD
	VALUE

	
	Form 
	
	
	Pasty

	
	Shade
	
	
	White

	
	Density (20ºC)
	(g/ml)
	EN ISO 2811.01-02
	0.33 ± 0.02

	
	Viscosity
	
	
	Thixotropic

	
	Painting after
	(min)
	
	20-30

	
	
	
	
	

	
	Note: Measurements are performed in a laboratory environment at a temperature of +230C, a Relative Humidity (RH) of 50% and without ventilation. Variations are possible depending on the work site conditions, such as temperature, humidity, ventilation and absorbency of the substrate.


	
	The technical information and guidelines in this brochure relating to the application and end-use of Thrakon’s products is based on the Company’s current expertise and experience on the products and are given in good faith provided they are properly stored, used and applied in accordance with the guidelines given by Thrakon. Given that we are unable to directly inspect the conditions that prevail at the work site as well as the application of the product, the Company shall not provide any guarantee regarding the suitability of its products for any particular purpose and disclaims any legal responsibility, which is based on written information in this brochure, written or oral or otherwise provided recommendations and guidelines. By applying the product is a small area, users are advised to test the product's suitability for the intended application and purpose. Thrakon reserves the right to amend the properties of its products without prior notice. All orders are accepted only after acceptance of the above and under the Company’s respective Trade Policy terms. This version of the technical data sheet automatically cancels any previous version.

	

	
	
	


